{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":3,"rows_kept":23,"merged":[[0,0,0,2],[2,0,2,2],[3,0,3,2],[4,0,5,0],[4,1,5,1],[4,2,5,2],[22,0,23,2]],"flags":["formulas_cached_only"]}
[]
[]
["BATTERY DATE CODE"]
["D126, D1218, D1224, D1238, D1240"]
["MANUFACTURER","DATE CODE","DESCRIPTION"]
[]
["MANTON, PANASONIC","YYMMDD","First two digits=year, next two digits=month, last two digits=day"]
["POWERSONIC","MMDDYY","First two digits=month, next two digits=day, last two digits=year"]
["TOYO, PANYU, HENDA, RADIONICS","HDYMMDD","First three digits= HDyear, next two digits=month, last two digits=day"]
{"$rows_empty":12}
["* NFPA72-2002, States to replace lead acid batteries five years after manufactured or sooner as needed"]
["Battery manufactures may change their date code scheme at anytime without notice. please refer to the battery manufacture if you have reason to believe this data to be inaccurate."]